The <a href="http://hdmi2usb.tv/numato-opsis">Numato Opsis</a>, the first open hardware for the
<a href="http://hdmi2usb.tv">HDMI2USB firmware</a>,
<a href="https://numato.com/product/numato-opsis-fpga-based-open-video-platform">can now be ordered
From Numato Labs
</a>

## Opsis Board - A open source HDMI2USB board

The [Numato](http://numato.com) Opsis board is the first
[HDMI2USB](http://hdmi2usb.tv) production board developed in conjugation with
the [TimVideos.us](http://code.timvideos.us) project. 

It's features include;
 * 2 x HDMI input ports,
 * 2 x HDMI output ports,
 * DisplayPort input and output ports,
 * 128Mbit DDR3-1600 ram,
 * Gigabit Ethernet with MAC address EEPROM,
 * Micro SD card,
 * Cypress FX2 for USB device functionality,
 * ULPI for USB OTG functionality,
 * Quad speed SPI flash.

Sample code for the Opsis can be found at https://github.com/timvideos/HDMI2USB-numato-opsis-sample-code

![Opsis V2 Prototype Picture](img/opsis-v2-prototype.jpg)

## Editing

The design in this repository was made using [KiCad](http://www.kicad-pcb.org/)
version **2013-07-07 BZR 4022**
([the version in Ubuntu Trusty](http://packages.ubuntu.com/trusty/kicad)).

## License

Opsis Board by Numato Systems Pvt. Ltd

The Numato HDMI2USB board is licensed under a
Creative Commons Attribution-ShareAlike 4.0 International License.

You should have received a copy of the license along with this
work. If not, see <http://creativecommons.org/licenses/by-sa/4.0/>.

![Creative Commons License Logo](https://i.creativecommons.org/l/by-sa/4.0/88x31.png)
