| Documentation For Arduino users

- Main Page
- Related Pages
- Modules
- Classes
- Files
- Examples

CompHotspot.ino

How to Use
  Show how to use API of class NexHotspot.

Author
  Wu Pengfei (email:pengf.nosp@m.ei.w.nosp@m.u@ite.nosp@m.ad.c.nosp@m.c)

Date
  2015/7/10

Copyright
  Copyright (C) 2014-2015 ITEAD Intelligent Systems Co., Ltd.
  This program is free software; you can redistribute it and/or modify it under the terms of the GNU General Public License as published by the Free Software Foundation; either version 2 of the License, or (at your option) any later version.

#include "Nextion.h"
NexHotspot hot0 = NexHotspot(0, 1, "hot0");
NexHotspot hot1 = NexHotspot(0, 2, "hot1");
NexTouch *nex_listen_list[] =
{
&hot0,
&hot1,
NULL
};
void hot0PushCallback(void *ptr)
{
dbSerialPrintln("hot0PushCallback");
dbSerialPrint("ptr=");
dbSerialPrintln((uint32_t)ptr);
}
void hot1PushCallback(void *ptr)
{
dbSerialPrintln("hot1PushCallback");
dbSerialPrint("ptr=");
dbSerialPrintln((uint32_t)ptr);
}
void hot0PopCallback(void *ptr)
{
dbSerialPrintln("hot0PopCallback");
dbSerialPrint("ptr=");
dbSerialPrintln((uint32_t)ptr);
}
void hot1PopCallback(void *ptr)
{
dbSerialPrintln("hot1PopCallback");
dbSerialPrint("ptr=");
dbSerialPrintln((uint32_t)ptr);
}
void setup(void)
{
nexInit();
hot0.attachPush(hot0PushCallback, &hot0);
hot0.attachPop(hot0PopCallback, &hot0);
hot1.attachPush(hot1PushCallback, &hot1);
hot1.attachPop(hot1PopCallback, &hot1);
dbSerialPrintln("setup done");
}
void loop(void)
{
nexLoop(nex_listen_list);
}