| Documentation For Arduino users

- Main Page
- Related Pages
- Modules
- Classes
- Files
- Examples

- File List
- File Members

CompSlider.ino
1
17 #include "Nextion.h"
18
19
20 NexText t0 = NexText(0, 2, "t0");
21 NexSlider h0 = NexSlider(0, 1, "h0");
22
23 NexTouch *nex_listen_list[] =
24 {
25 &h0,
26 NULL
27 };
28
29 void h0PopCallback(void *ptr)
30 {
31 uint32_t number = 0;
32 char temp[10] = {0};
33
34 dbSerialPrintln("h0PopCallback");
35
36 h0.getValue(&number);
37 utoa(number, temp, 10);
38 t0.setText(temp);
39 }
40
41
42 void setup(void)
43 {
44 nexInit();
45 h0.attachPop(h0PopCallback);
46 dbSerialPrintln("setup done");
47 }
48
49 void loop(void)
50 {
51 nexLoop(nex_listen_list);
52 }
53
nexLoop
void nexLoop(NexTouch *nex_listen_list[])
Listen touch event and calling callbacks attached before.
Definition: NexHardware.cpp:235
NexSlider
NexSlider component.
Definition: NexSlider.h:30
NexText::setText
bool setText(const char *buffer)
Set text attribute of component.
Definition: NexText.cpp:32
NexSlider::getValue
bool getValue(uint32_t *number)
Get the value of slider.
Definition: NexSlider.cpp:22
NexTouch::attachPop
void attachPop(NexTouchEventCb pop, void *ptr=NULL)
Attach an callback function of pop touch event.
Definition: NexTouch.cpp:39
nexInit
bool nexInit(void)
Init Nextion.
Definition: NexHardware.cpp:220
Nextion.h
The header file including all other header files provided by this library.
NexTouch
Father class of the components with touch events.
Definition: NexTouch.h:53
NexText
NexText component.
Definition: NexText.h:30