(footprint "60x180 SPI Disp 0.96in" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61EA18FB)
  (attr smd)
  (fp_text reference "REF**" (at 15.24 -12.7 unlocked) (layer "F.SilkS"))
  (fp_text value "60x180 SPI Disp 0.96in" (at 15.24 -10.16 unlocked) (layer "F.Fab"))
  (fp_text user "GND" (at 6.1 -20.6 unlocked) (layer "F.SilkS"))
  (fp_text user "CS" (at 21.3 -20.6 unlocked) (layer "F.SilkS"))
  (fp_text user "SDA" (at 13.7 -20.6 unlocked) (layer "F.SilkS"))
  (fp_text user "SCL" (at 11.1 -20.6 unlocked) (layer "F.SilkS"))
  (fp_text user "DC" (at 18.8 -20.6 unlocked) (layer "F.SilkS"))
  (fp_text user "RES" (at 16.2 -20.6 unlocked) (layer "F.SilkS"))
  (fp_text user "VCC" (at 8.6 -20.6 unlocked) (layer "F.SilkS"))
  (fp_text user "BLK" (at 23.9 -20.6 unlocked) (layer "F.SilkS"))
  (fp_text user "80x160 SPI Disp 0.96\"" (at 15.1 -2.6 unlocked) (layer "F.SilkS"))
  (fp_text user "${REFERENCE}" (at 15.24 -12.7 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 6.11 -22.6) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 8.65 -22.6) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at 11.19 -22.6) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at 13.73 -22.6) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at 16.27 -22.6) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad "6" thru_hole circle (at 18.81 -22.6) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad "7" thru_hole circle (at 21.35 -22.6) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad "8" thru_hole circle (at 23.89 -22.6) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at 27.4 -2.57) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at 2.6 -2.57) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at 2.6 -21.37) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at 27.4 -21.37) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask))
)
