(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 93)
    (no_connects 0)
    (area 39.949999 29.949999 140.050001 110.050001)
    (thickness 1.6)
    (drawings 6)
    (tracks 388)
    (zones 0)
    (modules 26)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.8128)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory PUCONMP575ACMA001_Fab/))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GNDD)
  (net 3 "Net-(J1-Pad3)")
  (net 4 /D13)
  (net 5 /D14)
  (net 6 /D12)
  (net 7 /D25)
  (net 8 /TX0)
  (net 9 /D26)
  (net 10 /RX0)
  (net 11 /D35)
  (net 12 /TX2)
  (net 13 /VN)
  (net 14 /RX2)
  (net 15 /VP)
  (net 16 /D2)
  (net 17 /EN)
  (net 18 +3V3)
  (net 19 /DRV_FEED)
  (net 20 /DRV_COLOR)
  (net 21 /DRV_MOTOR)
  (net 22 /DRV_M6)
  (net 23 /DRV_M5)
  (net 24 /SNS_ROT)
  (net 25 /DRV_M4)
  (net 26 /SNS_HOME)
  (net 27 /DRV_M3)
  (net 28 "Net-(J3-Pad2)")
  (net 29 /DRV_M2)
  (net 30 +5V)
  (net 31 /DRV_M1)
  (net 32 /DRV_M0)
  (net 33 /CTL_M6)
  (net 34 /CTL_M5)
  (net 35 /CTL_M4)
  (net 36 /CTL_M3)
  (net 37 /CTL_M2)
  (net 38 /CTL_M1)
  (net 39 /CTL_COLOR)
  (net 40 /CTL_M0)
  (net 41 /CTL_MOTOR)
  (net 42 /CTL_FEED)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CTL_COLOR)
    (add_net /CTL_FEED)
    (add_net /CTL_M0)
    (add_net /CTL_M1)
    (add_net /CTL_M2)
    (add_net /CTL_M3)
    (add_net /CTL_M4)
    (add_net /CTL_M5)
    (add_net /CTL_M6)
    (add_net /CTL_MOTOR)
    (add_net /D12)
    (add_net /D13)
    (add_net /D14)
    (add_net /D2)
    (add_net /D25)
    (add_net /D26)
    (add_net /D35)
    (add_net /EN)
    (add_net /RX0)
    (add_net /RX2)
    (add_net /SNS_HOME)
    (add_net /SNS_ROT)
    (add_net /TX0)
    (add_net /TX2)
    (add_net /VN)
    (add_net /VP)
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J3-Pad2)")
  )
  (net_class Driver ""
    (clearance 0.5)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DRV_COLOR)
    (add_net /DRV_FEED)
    (add_net /DRV_M0)
    (add_net /DRV_M1)
    (add_net /DRV_M2)
    (add_net /DRV_M3)
    (add_net /DRV_M4)
    (add_net /DRV_M5)
    (add_net /DRV_M6)
    (add_net /DRV_MOTOR)
  )
  (net_class Power ""
    (clearance 0.5)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net GNDD)
  )
  (module Footprints:DIP-4_1_ELL (layer F.Cu) (tedit 0)
    (at 57.785 61.595)
    (fp_text reference U1 (at -12.84 0 90) (layer F.SilkS))
    (fp_text value DCstepDownConvADJLM2596 (at 0 0) (layer F.Fab))
    (pad 4 thru_hole oval (at -8.89 -20.32) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 +5V))
    (pad 1 thru_hole oval (at -8.89 20.32) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 3 thru_hole oval (at 8.89 -20.32) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (pad 2 thru_hole oval (at 8.89 20.32) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model Converters_DCDC_ACDC.3dshapes/DCDC-Conv_TRACO_TSR-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Barrel_Jack_CUI_PJ-102AH (layer F.Cu) (tedit 59BC552D)
    (at 53.975 92.71 270)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J1 (at 5.75 8.45 360) (layer F.SilkS))
    (fp_text value Power_12V_DV (at -5.5 6.2 360) (layer F.Fab))
    (fp_text user %R (at 0 6.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 0 6 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (pad 3 thru_hole circle (at 4.7 3 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Barrel_Jack_CUI_PJ-102AH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:PinHeader_0.6mmSquare_01x16_2.54mm (layer F.Cu) (tedit 5AC15977)
    (at 105.41 34.29)
    (fp_text reference J2 (at 0 -2.54) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at 0 2.54) (layer F.Fab))
    (pad 8 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 /D13))
    (pad 9 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 /D14))
    (pad 7 thru_hole circle (at -3.81 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 /D12))
    (pad 10 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /D25))
    (pad 6 thru_hole circle (at -6.35 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /TX0))
    (pad 11 thru_hole circle (at 6.35 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 /D26))
    (pad 5 thru_hole circle (at -8.89 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 /RX0))
    (pad 12 thru_hole circle (at 8.89 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 /D35))
    (pad 4 thru_hole circle (at -11.43 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 /TX2))
    (pad 13 thru_hole circle (at 11.43 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 /VN))
    (pad 3 thru_hole circle (at -13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 /RX2))
    (pad 14 thru_hole circle (at 13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 /VP))
    (pad 2 thru_hole circle (at -16.51 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 /D2))
    (pad 15 thru_hole circle (at 16.51 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /EN))
    (pad 1 thru_hole rect (at -19.05 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 16 thru_hole circle (at 19.05 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GNDD))
  )
  (module Footprints:PinHeader_Female_0.6mmSquare_01x18_2.54mm (layer F.Cu) (tedit 5AC157CE)
    (at 106.68 103.505 180)
    (fp_text reference J3 (at -2.54 -2.54 180) (layer F.SilkS))
    (fp_text value Print_Mech_Citizen_MP575 (at -2.54 2.54 180) (layer F.Fab))
    (pad 8 thru_hole circle (at -3.81 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 /DRV_FEED))
    (pad 9 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 /DRV_COLOR))
    (pad 7 thru_hole circle (at -6.35 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 10 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 6 thru_hole circle (at -8.89 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 /DRV_MOTOR))
    (pad 11 thru_hole circle (at 3.81 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 /DRV_M6))
    (pad 5 thru_hole circle (at -11.43 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (pad 12 thru_hole circle (at 6.35 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /DRV_M5))
    (pad 4 thru_hole circle (at -13.97 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 /SNS_ROT))
    (pad 13 thru_hole circle (at 8.89 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 /DRV_M4))
    (pad 3 thru_hole circle (at -16.51 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 /SNS_HOME))
    (pad 14 thru_hole circle (at 11.43 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 /DRV_M3))
    (pad 2 thru_hole circle (at -19.05 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad2)"))
    (pad 15 thru_hole circle (at 13.97 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 /DRV_M2))
    (pad 1 thru_hole rect (at -21.59 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 +5V))
    (pad 16 thru_hole circle (at 16.51 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 /DRV_M1))
    (pad 17 thru_hole circle (at 19.05 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 /DRV_M0))
    (pad 18 thru_hole circle (at 21.59 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 +3V3))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 100.33 90.805 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference Q1 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value IRF7301PbF (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /CTL_M6))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /CTL_M5))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /DRV_M5))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /DRV_M5))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /DRV_M6))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /DRV_M6))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 114.3 90.805 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference Q2 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value IRF7301PbF (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /CTL_M4))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /CTL_M3))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /DRV_M3))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /DRV_M3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /DRV_M4))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /DRV_M4))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 93.345 90.805 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference Q3 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value IRF7301PbF (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /CTL_M2))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /CTL_M1))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /DRV_M1))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /DRV_M1))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /DRV_M2))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /DRV_M2))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 85.09 90.805 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference Q4 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value IRF7301PbF (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /CTL_COLOR))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /CTL_M0))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /DRV_M0))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /DRV_M0))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /DRV_COLOR))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /DRV_COLOR))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 107.315 90.805 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference Q5 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value IRF7301PbF (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /CTL_MOTOR))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /CTL_FEED))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /DRV_FEED))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /DRV_FEED))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /DRV_MOTOR))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /DRV_MOTOR))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 106.045 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /CTL_M6))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 118.745 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /CTL_M2))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 94.615 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /CTL_FEED))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 109.855 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /CTL_M0))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 130.175 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /CTL_M4))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 126.365 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /CTL_M3))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 114.3 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /CTL_M1))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 102.235 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /CTL_M5))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 98.425 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /CTL_MOTOR))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 122.555 62.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /CTL_COLOR))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 123.19 85.09 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /SNS_HOME))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 132.08 85.09 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /SNS_ROT))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:DOITESP32DEVKIT (layer F.Cu) (tedit 0)
    (at 112.395 57.785)
    (fp_text reference U2 (at -27.615 0 90) (layer F.SilkS))
    (fp_text value DOITESP32DEVKIT (at 0 0) (layer F.Fab))
    (pad 30 thru_hole oval (at -17.78 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 +5V))
    (pad 1 thru_hole oval (at -17.78 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 29 thru_hole oval (at -15.24 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (pad 2 thru_hole oval (at -15.24 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDD))
    (pad 28 thru_hole oval (at -12.7 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D13))
    (pad 3 thru_hole oval (at -12.7 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /CTL_MOTOR))
    (pad 27 thru_hole oval (at -10.16 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D12))
    (pad 4 thru_hole oval (at -10.16 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /D2))
    (pad 26 thru_hole oval (at -7.62 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D14))
    (pad 5 thru_hole oval (at -7.62 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /CTL_M5))
    (pad 25 thru_hole oval (at -5.08 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /CTL_FEED))
    (pad 6 thru_hole oval (at -5.08 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /RX2))
    (pad 24 thru_hole oval (at -2.54 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D25))
    (pad 7 thru_hole oval (at -2.54 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /TX2))
    (pad 23 thru_hole oval (at 0 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D26))
    (pad 8 thru_hole oval (at 0 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /CTL_M6))
    (pad 22 thru_hole oval (at 2.54 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /SNS_HOME))
    (pad 9 thru_hole oval (at 2.54 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /CTL_M0))
    (pad 21 thru_hole oval (at 5.08 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /CTL_COLOR))
    (pad 10 thru_hole oval (at 5.08 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /CTL_M1))
    (pad 20 thru_hole oval (at 7.62 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /D35))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /CTL_M2))
    (pad 19 thru_hole oval (at 10.16 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /SNS_ROT))
    (pad 12 thru_hole oval (at 10.16 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /RX0))
    (pad 18 thru_hole oval (at 12.7 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VN))
    (pad 13 thru_hole oval (at 12.7 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /TX0))
    (pad 17 thru_hole oval (at 15.24 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /VP))
    (pad 14 thru_hole oval (at 15.24 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /CTL_M3))
    (pad 16 thru_hole oval (at 17.78 -12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /EN))
    (pad 15 thru_hole oval (at 17.78 12.7) (size 1.27 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /CTL_M4))
  )
  (module Footprints:TP_Mounthole_3.2mm (layer F.Cu) (tedit 5AC7FF2C)
    (at 46 104)
    (fp_text reference TP1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value TEST (at 0 3.81) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Footprints:TP_Mounthole_3.2mm (layer F.Cu) (tedit 5AC7FF2C)
    (at 134 104)
    (fp_text reference TP2 (at 0 -3.81) (layer F.SilkS))
    (fp_text value TEST (at 0 3.81) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Footprints:TP_Mounthole_3.2mm (layer F.Cu) (tedit 5AC7FF2C)
    (at 45 35)
    (fp_text reference TP3 (at 0 -3.81) (layer F.SilkS))
    (fp_text value TEST (at 0 3.81) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Footprints:TP_Mounthole_3.2mm (layer F.Cu) (tedit 5AC7FF2C)
    (at 135 35)
    (fp_text reference TP4 (at 0 -3.81) (layer F.SilkS))
    (fp_text value TEST (at 0 3.81) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text PUCONMP575ACBA001 (at 63.075 35.95) (layer B.SilkS))
  (gr_text PUCONMP575ACBA001 (at 63.15 32.825) (layer F.SilkS))
  (gr_line (start 40 110) (end 40 30) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140 110) (end 40 110) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140 30) (end 140 110) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40 30) (end 140 30) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.192 109.22) (xy 40.64 109.22) (xy 40.64 30.48) (xy 139.192 30.48)
      )
    )
  )
)
