
This directory contains designs for mounting the Numato Opsis in cases.

This git repository is the master but the designs can also be found on
[Thingiverse](http://www.thingiverse.com/groups/timvideos/things).

 * `layout` - Designs showing the port size and locations to enable easy case construction.
 * `layout/front.svg` - Front of the board containing the HDMI, USB-B and DisplayPort connectors.
 * (TODO) `layout/back.svg` - Back of the board containing the Ethernet, Micro USB and power connectors.
 * (TODO) `layout/side.svg` - Side of the board containing the MicroSD slot.

 * `io-shield` - IO shields designed to fit ready made cases.

 * `io-shield/atx` - Fits an standard ATX case.

 * `io-shield/inset-thin` - Fits the
   [Inset Technologies "Thin Mini-ITX Computer Case"](http://amzn.to/1Okez89)
   when used with
   [#6-32 to M3 Metal Standoffs](http://amzn.to/2anqXwz).

 * `(.*)-mouse-ears.stl` - Same as `\1.stl`, but with 'mouse-ears' to aid 3d printing.

