| Documentation For Arduino users

- Main Page
- Related Pages
- Modules
- Classes
- Files
- Examples

- File List
- File Members

NexPicture.h
Go to the documentation of this file.
1
17 #ifndef __NEXPICTURE_H__
18 #define __NEXPICTURE_H__
19
20 #include "NexTouch.h"
21 #include "NexHardware.h"
30 class NexPicture: public NexTouch
31 {
32 public: /* methods */
36 NexPicture(uint8_t pid, uint8_t cid, const char *name);
37
46 bool getPic(uint32_t *number);
47
56 bool setPic(uint32_t number);
57 };
58
63 #endif /* #ifndef __NEXPICTURE_H__ */
NexPicture::setPic
bool setPic(uint32_t number)
Set picture's number.
Definition: NexPicture.cpp:32
NexPicture
NexPicture component.
Definition: NexPicture.h:30
NexTouch.h
The definition of class NexTouch.
NexHardware.h
The definition of base API for using Nextion.
NexPicture::NexPicture
NexPicture(uint8_t pid, uint8_t cid, const char *name)
Constructor.
Definition: NexPicture.cpp:18
NexPicture::getPic
bool getPic(uint32_t *number)
Get picture's number.
Definition: NexPicture.cpp:23
NexTouch
Father class of the components with touch events.
Definition: NexTouch.h:53