| Documentation For Arduino users

- Main Page
- Related Pages
- Modules
- Classes
- Files
- Examples

CompCrop.ino

How to Use
  Show how to use API of class NexCrop.

Author
  Wu Pengfei (email:pengf.nosp@m.ei.w.nosp@m.u@ite.nosp@m.ad.c.nosp@m.c)

Date
  2015/7/10

Copyright
  Copyright (C) 2014-2015 ITEAD Intelligent Systems Co., Ltd.
  This program is free software; you can redistribute it and/or modify it under the terms of the GNU General Public License as published by the Free Software Foundation; either version 2 of the License, or (at your option) any later version.

#include "Nextion.h"
NexCrop q0 = NexCrop(0, 1, "q0");
NexTouch *nex_listen_list[] =
{
&q0,
NULL
};
void q0PopCallback(void *ptr)
{
uint32_t number = 0;
dbSerialPrintln("q0PopCallback");
q0.getPic(&number);
number += 1;
number %= 2;
q0.setPic(number);
}
void setup(void)
{
nexInit();
q0.attachPop(q0PopCallback);
dbSerialPrintln("setup done");
}
void loop(void)
{
nexLoop(nex_listen_list);
}